Name: TOP10LT-SR

Scale: 1:10000

Territory: 2 sheets of Vilnius City

Format: TIFF

Coordinate system: LKS94 (Lithuanian Coordinate System) 

Colorful Raster Data Bases TOP10LT-SR for the Lithuanian Topographic Map at scale 1:10000  for this moment this data base is prepared for Vilnius, Kaunas and Marijampolė cities, Kaišiadorys, Elektrėnai, Trakai municipalities (6300 square meters).
TOP10LT-SR is created with the help of vector - raster conversion process, using midi level of Cartographic Data Base of the Lithuanian Topographic Map KDB10LT at scale 1:10000.

More information you can find on the web site: http://www.gis-centras.lt/gisweb/index.php?pageid=255